

MAD CONTROL BOARD MODS REQUIRED

On the left side of the PCB the track on the top layer needs to be cut as per below and a connection made as shown in white.



Near the power switch connector cut the 3 tracks on the bottom as shown with X, change the left resistor from 1K to 10K. When fitting the components you can then use the extra wire on the legs to make the connections shown in white.



The 2 components circled in red below are different to what is shown on the silk screen. The 1K resistors was shown as 4k3 and the 22nf capacitor was 1n.

